{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1"]
["","Kasutusjuhend","","","","1"]
["","Ühendustorud","","","","1"]
["","F-gaasi määruse kohane jahutusainesilt","","","","1"]
["","Külmutusagensi täitmise silt","","","","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","1"]
["Kaal","Ühik","","","kg","370"]
["Külmaaine","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Charge","","","kg","11.5"]
["","Tüüp","","","","R-410A"]
["Ventilaatori mootor","Väljundvõimsus","","","W","750"]
["","Ajam","","","","Otseajam"]
["Soojusvaheti","Tüüp","","","","Ristribidega spiraal"]
["Mõõtmed","Ühik","","Laius","mm","1,240"]
["","","","Sügavus","mm","765"]
["","","","Kõrgus","mm","1,680"]
["Korpus","Värvus","","","","Elevandiluuvalge"]
["Ventilaator","Tüüp","","","","Tiivikventilaator"]
["","Õhu vooluhulk","Jahutus","Nom","m³/min","230"]
["","Kogus","","","","2"]
["Power supply","Faas","","","","3~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","380-415"]
["Märkused","","","","","(1) - Jahutuse prioriteetrežiimis: sisetemperatuur 27 °CDB, 19 °CWB; välistemp. 32 °CDB; torustiku pikkus: 7,5m; kõrguste vahe: 0m"]
["","","","","","(2) - Jahutuse prioriteetrežiimis: aurustustemperatuur -10°C; välistemp. 32 °CDB; Imu SH: 10°C"]
["","","","","","(3) - Soojustagastus 100% režiim: sisetemperatuur 20 °CDB; välistemp. 7 °CDB, 6 °CWB; jahutuskoormus 18 kW; torustiku pikkus: 7,5m; kõrguste vahe: 0m"]
["","","","","","(4) - Imirõhuga ekvivalentne küllastunud temperatuur (jahutuspool): -10 °C (jahutatud tingimustes); Siseruumi õhukonditsioneeri ühendusvõimsus: 10 hj, kui soojustagastus on 100%"]
["","","","","","(5) - Kompressor 1"]
["","","","","","(6) - Kompressor 2"]
["","","","","","(7) - Kompressor 3"]
["","","","","","(8) - Seadme tehasetäide"]
["","","","","","(9) - Paigaldage õlilukk 5 m kaugusele välisseadmest"]
["","","","","","(10) - Enama teabe sammiseks vt talitlusvahemiku joonist"]
["","","","","","(11) - Enamat teavet standardsete lisaseadmete kohta vt paigaldamis- ja kasutusjuhendist."]
["","","","","","(12) - Sisaldav fluoritud kasvuhoonegaase"]