{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC30YV"]
[]
[]
[]
[]
["","","","","","MC30YVM"]
["Tüüp","","","","","Õhupuhasti"]
["Rakendus","","","","","Põrandal seisev tüüp"]
["Korpus","Värvus","","","","Valge"]
["Mõõtmed","Seade","","Kõrgus","mm","450"]
["","","","Laius","mm","270"]
["","","","Sügavus","mm","270"]
["Kaal","Ühik","","","kg","5.8"]
["Sobiv ruumi pindala","m²","","","","23 (1), 46 (2)"]
["CADR","m³/h","","","","180"]
["Õhupuhastus","Sisendvõimsus","","Turbo","kW","0.025"]
["","","","M","kW","0.015"]
["","","","Vaikne","kW","0.008"]
["Mürarõhutase","Õhupuhastus","","Turbo","dBA","37"]
["","","","keskmine","dBA","27"]
["","","","Vaikne","dBA","19"]
["Ventilaator","Õhu vooluhulk","Õhupuhastus","Turbo","m³/h","180"]
["","","","keskmine","m³/h","120"]
["","","","Vaikne","m³/h","60"]
["Tolmukogumismeetod","","","","","Elektrostaatiline HEPA-filter"]
["Desodoreerimismeetod","","","","","Flash-striimer + deodoreeriv katalüsaator"]
["Standardsed lisatarvikud","Elektrostaatiline HEPA-filter","","","","1"]
["","Deodoriseeriv filter","","","","1"]
["","Kasutusjuhend","","","","1"]
["Toitejuhe","m","","","","1.8"]
["Power supply","Faas","","","","1~"]
["","Sagedus","","","Hz","50/60"]
["","Pinge","","","V","220-240/220-230"]
["Töövool","Õhupuhastus","","Turbo","A","0.13"]
["","","","keskmine","A","0.09"]
["","","","Vaikne","A","0.08"]
["Märkused","","","","","(1) - Kohaldatav ruumi pindala vastab ventilaatori maksimaalsel kiirusel (HH) töötavale seadmele. Kohaldatav ruumi pindala tähistab ruumi, kus 30 minutiga on võimalik eemaldada teatud koguse tolmuosakesi. (JEM 1467)"]
["","","","","","(2) - Kohaldatav ruumi pindala vastab ventilaatori maksimaalsel kiirusel (HH) töötavale seadmele. See arvutati vastavalt standardile NRCC-54013, kasutades sigarisuitsu CADRi, mida katsetati vastavalt standardile JEM1467."]
["","","","","","(3) - Katseväärtustest teisendatud CADR standarditele vastavalt standardile JEM1467."]
["","","","","","(4) - Töötamismüratasemed on keskmised väärtused, mis on mõõdetud seadme esiosast, vasakust ja paremast küljest ning pealmisest osast 1 m kaugusel. (Võrduvad kajavabas testkambris mõõdetud väärtusega)"]
["","","","","","(5) - Elektrostaatiline HEPA-filter on kinnitatud seadmele."]
["","","","","","(6) - Muu funktsioon: Automaatse taaskäivitamise funktsioon."]