{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Tüüp","","","","","Niisutav õhupuhasti"]
["Rakendus","","","","","Põrandal seisev tüüp"]
["Korpus","Värvus","","","","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","700"]
["","","","Laius","mm","270"]
["","","","Sügavus","mm","270"]
["Kaal","Ühik","","","kg","9.5"]
["Sobiv ruumi pindala","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Õhupuhastus","Sisendvõimsus","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Vaikne","kW","0.007"]
["Niiskusrežiim","Sisendvõimsus","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Vaikne","kW","0.011"]
["","Veepaagi maht","","","l","2.7"]
["Mürarõhutase","Õhupuhastus","","Turbo","dBA","53.0"]
["","","","keskmine","dBA","39.0"]
["","","","aeglane","dBA","29.0"]
["","","","Vaikne","dBA","19.0"]
["","Niiskusrežiim","","Turbo","dBA","53.0"]
["","","","keskmine","dBA","39.0"]
["","","","aeglane","dBA","33.0"]
["","","","Vaikne","dBA","25.0"]
["Ventilaator","Õhu vooluhulk","Õhupuhastus","Turbo","m³/h","330"]
["","","","keskmine","m³/h","192"]
["","","","aeglane","m³/h","120"]
["","","","Vaikne","m³/h","54"]
["","","Niiskusrežiim","Turbo","m³/h","330"]
["","","","keskmine","m³/h","192"]
["","","","aeglane","m³/h","144"]
["","","","Vaikne","m³/h","102"]
["Tolmukogumismeetod","","","","","Elektrostaatiline HEPA-filter"]
["Desodoreerimismeetod","","","","","Flash-striimer + deodoreeriv katalüsaator"]
["Standardsed lisatarvikud","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Toitejuhe","Toitejuhe","","","","1.8"]
["Elektritoide","Faas","","","","1~"]
["","Elektritoide-=-Sagedus","","Sagedus","","50/60"]
["","Elektritoide-=-Pinge","","Pinge","","220-240/220-230"]
["Töövool","Õhupuhastus","Töövool-=-Õhupuhastus-=-Turbo","Turbo","","0.50"]
["","","Töövool-=-Õhupuhastus-=-keskmine","keskmine","","0.19"]
["","","Töövool-=-Õhupuhastus-=-aeglane","aeglane","","0.12"]
["","","Töövool-=-Õhupuhastus-=-Vaikne","Vaikne","","0.09"]
["","Niiskusrežiim","Töövool-=-Niiskusrežiim-=-Turbo","Turbo","","0.50"]
["","","Töövool-=-Niiskusrežiim-=-keskmine","keskmine","","0.20"]
["","","Töövool-=-Niiskusrežiim-=-aeglane","aeglane","","0.15"]
["","","Töövool-=-Niiskusrežiim-=-Vaikne","Vaikne","","0.13"]
["Märkused","","","","","(1) - Kohaldatav ruumi pindala vastab ventilaatori maksimaalsel kiirusel (HH) töötavale seadmele. Kohaldatav ruumi pindala tähistab ruumi, kus 30 minutiga on võimalik eemaldada teatud koguse tolmuosakesi. (JEM 1467)"]
["","","","","","(2) - Katseväärtustest teisendatud NRCC standarditele vastavalt standardile JEM1467."]