{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Tüüp","","","","","Niisutav õhupuhasti"]
["Rakendus","","","","","Põrandal seisev tüüp"]
["Korpus","Värvus","","","","Valge (N9. 0)"]
["Mõõtmed","Ühik","","Kõrgus","mm","600 (5)"]
["","","","Laius","mm","395"]
["","","","Sügavus","mm","287"]
["Kaal","Ühik","","","kg","12.5"]
["Sobiv ruumi pindala","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Õhupuhastus","Sisendvõimsus","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Vaikne","kW","0.008"]
["Niiskusrežiim","Sisendvõimsus","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Vaikne","kW","0.011"]
["","Veepaagi maht","","","l","3.6"]
["Mürarõhutase","Õhupuhastus","","Turbo","dBA","54"]
["","","","keskmine","dBA","37"]
["","","","aeglane","dBA","27"]
["","","","Vaikne","dBA","18"]
["","Niiskusrežiim","","Turbo","dBA","54"]
["","","","keskmine","dBA","37"]
["","","","aeglane","dBA","27"]
["","","","Vaikne","dBA","23"]
["Ventilaator","Õhu vooluhulk","Õhupuhastus","Turbo","m³/h","420"]
["","","","keskmine","m³/h","210"]
["","","","aeglane","m³/h","132"]
["","","","Vaikne","m³/h","60"]
["","","Niiskusrežiim","Turbo","m³/h","420"]
["","","","keskmine","m³/h","210"]
["","","","aeglane","m³/h","132"]
["","","","Vaikne","m³/h","102"]
["Tolmukogumismeetod","","","","","Elektrostaatiline HEPA-filter"]
["Desodoreerimismeetod","","","","","Flash-striimer + deodoreeriv katalüsaator"]
["Standardsed lisatarvikud","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Toitejuhe","m","","","","2"]
["Elektritoide","Faas","","","","1~"]
["","Sagedus","","","Hz","50/60"]
["","Pinge","","","V","220-240/220-230"]
["Märkused","","","","","(1) - Kaetav pindala vastab ventilaatori maksimaalsel kiirusel (HH) töötavale seadmele. Kaetav pindala tähistab ruumi, kus teatud kogus tolmuosakesi eemaldatakse 30 minutiga."]
["","","","","","(2) - Katseväärtustest teisendatud NRCC standarditele vastavalt standardile JEM1467."]
["","","","","","(3) - Töötamismüratasemed on keskmised väärtused, mis on mõõdetud seadme esiosast, vasakust ja paremast küljest ning pealmisest osast 1 m kaugusel. (Võrduvad kajavabas testkambris mõõdetud väärtusega)"]