{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":16,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A"]
[]
[]
[]
[]
["","","","","","RXA20A2V1B","RXA20A3V1B","RXA20A5V1B","RXA25A2V1B","RXA25A3V1B","RXA25A5V1B","RXA35A2V1B","RXA35A3V1B","RXA35A5V1B","RXA42A2V1B","RXA50A2V1B"]
["Mõõtmed","Ühik","","Kõrgus","mm","550","550","550","550","550","550","550","550","550","735","735"]
["","","","Laius","mm","765","765","765","765","765","765","765","765","765","825","825"]
["","","","Sügavus","mm","285","285","285","285","285","285","285","285","285","300","300"]
["Kaal","Ühik","","","kg","32","32","32","32","32","32","32","32","32","46","46"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max","° CDB","46","46","46","46","46","46","46","46","46","46","46"]
["","Küte","Keskkond","Min","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max","°CWB","18","18","18","18","18","18","18","18","18","18","18"]
["Mürarõhutase","Jahutus","","Nom","dBA","46","46","46","46","46","46","49","49","49","48","48"]
["","Küte","","Nom","dBA","47","47","47","47","47","47","49","49","49","48","48"]
["Külmaaine","Tüüp","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Kogus","","","kg","0.76","0.76","0.76","0.76","0.76","0.76","0.76","0.76","0.76","1.30","1.30"]
["","Kogus","","","tCO2Eq","0.52","0.52","0.52","0.52","0.52","0.52","0.52","0.52","0.52","0.88","0.88"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20","20","20","20","20","20","20","20","20","30","30"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15.0","15.0","15.0","15.0","15.0","15.0","15.0","15.0","15.0","20.0","20.0"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1","1","1","1"]
["Elektritoide","Faas","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50","50","50","50","50","50","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]