{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A8"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B8","RXA25A5V1B8","RXA35A5V1B8"]
["Mõõtmed","Ühik","","Kõrgus","mm","550","550","550"]
["","","","Laius","mm","840","840","840"]
["","","","Sügavus","mm","350","350","350"]
["Kaal","Ühik","","","kg","32","32","32"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10","-10","-10"]
["","","","Max","°CDB","46","46","46"]
["","Küte","Keskkond","Min","°CWB","-15","-15","-15"]
["","","","Max","°CWB","18","18","18"]
["Mürarõhutase","Jahutus","","Nom","dBA","46.0","46.0","49.0"]
["","Küte","","Nom","dBA","47.0","47.0","49.0"]
["Külmaaine","Tüüp","","","","R-32","R-32","R-32"]
["","Kogus","","","kg","0.76","0.76","0.76"]
["","Kogus","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675.0","675.0","675.0"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20","20","20"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15.0","15.0","15.0"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Energiatõhususe klass","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Elektritoide","Faas","","","","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240"]
["Märkused","","","","","(1) - Sisaldav fluoritud kasvuhoonegaase","(1) - Sisaldav fluoritud kasvuhoonegaase","(1) - Sisaldav fluoritud kasvuhoonegaase"]
["","","","","","(2) - Vt töövahemiku kohta eraldi joonist","(2) - Vt töövahemiku kohta eraldi joonist","(2) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","(3) - Vt eraldi elektriandmete joonist","(3) - Vt eraldi elektriandmete joonist","(3) - Vt eraldi elektriandmete joonist"]