{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B5V1B","RXA42B2V1B","RXA50B5V1B","RXA50B2V1B"]
["Mõõtmed","Ühik","","Kõrgus","mm","","734","734","734"]
["","","","Laius","mm","","870","954","870"]
["","","","Sügavus","mm","","373","401","373"]
["Kaal","Ühik","","","kg","","50","49","50"]
["Kompressor","Tüüp","","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","","-10","-10","-10"]
["","","","Max","°CDB","","46","46","46"]
["","Küte","Keskkond","Min","°CWB","","-15","-15","-15"]
["","","","Max","°CWB","","18","18","18"]
["Mürarõhutase","Jahutus","","Nom","dBA","","48.0","48","48.0"]
["","Küte","","Nom","dBA","","48.0","48","48.0"]
["Külmaaine","Tüüp","","","","","R-32","R-32","R-32"]
["","Kogus","","","kg","","1.10","1.1","1.10"]
["","Kogus","","","tCO2Eq","","0.75","0.75","0.75"]
["","GWP","","","","","675","675","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","","30","30","30"]
["","Jahutusaine lisatäide","","","kg/m","","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","","20","20","20"]
["Energiatõhususe klass","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Elektritoide","Faas","","","","","1~","1~","1~"]
["","Sagedus","","","Hz","","50","50","50"]
["","Pinge","","","V","","220-240","220-240","220-240"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","","1","1","1"]
["","Külmutusagensi täitmise silt","","","","","1","1","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","","1","1","1"]
["","Tühjendusava kate","","","","","3","3","3"]
["","Tühjendusava kork","","","","","1","1","1"]
["Märkused","","","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist"]
["","","","","","","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase"]