{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-N"]
[]
[]
[]
[]
["","","","","","RXJ50N2V1B"]
["Mõõtmed","Ühik","","Kõrgus","mm","734"]
["","","","Laius","mm","870"]
["","","","Sügavus","mm","373"]
["Kaal","Ühik","","","kg","50"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10"]
["","","","Max","°CDB","46"]
["","Küte","Keskkond","Min","°CWB","-15"]
["","","","Max","°CWB","18"]
["Mürarõhutase","Jahutus","","Nom","dBA","48.0"]
["","Küte","","Nom","dBA","48.0"]
["Külmaaine","Tüüp","","","","R-32"]
["","Kogus","","","kg","1.15"]
["","Kogus","","","tCO2Eq","0.78"]
["","GWP","","","","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","30"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","20"]
["Standardsed lisatarvikud","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["Elektritoide","Faas","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","220-240"]