{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","30.6","30.6"]
["","","Soojendamine","Ülimadal","m³/min","27.2","27.2"]
["","","","Ülimadal","cfm","1080","1080"]
["","","Soojendamine","Ülimadal","cfm","960","960"]
["Mõõtmed","Ühik","","Kõrgus","mm","550","550"]
["","","","Laius","mm","858","858"]
["","","","Sügavus","mm","330","330"]
["Kaal","Ühik","","","kg","40","40"]
["Kompressor","Tüüp","","","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","-10","-10"]
["","","","Max","° CDB","46","46"]
["","Küte","Keskkond","Min","°CWB","-25","-25"]
["","","","Max","°CWB","18","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","48","48"]
["","","","aeglane","dBA","44","44"]
["","Küte","","kiire","dBA","49","49"]
["","","","aeglane","dBA","45","45"]
["Külmaaine","Tüüp","","","","R-410A","R-410A"]
["","Kogus","","","kg","1","1"]
["","Kogus","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20","20"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - IU","Max","m","15","15"]
["Standardsed lisatarvikud","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Elektritoide","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor"]