{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":16,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A"]
[]
[]
[]
[]
["","","","","","RXM20A5V1B","RXM25A5V1B","RXM35A5V1B","RXM42A5V1B","RXM50A5V1B","RXM60A2V1B","RXM60A5V1B","RXM71A2V1B","RXM71A5V1B","RXM42A2V1B (Archived)"]
["Mõõtmed","Ühik","","Kõrgus","mm","610","610","610","610","734","","734","","734"]
["","","","Laius","mm","923","923","923","923","954","","954","","954"]
["","","","Sügavus","mm","367","367","367","367","401","","401","","401"]
["Kaal","Ühik","","","kg","36","36","36","40","49","","49","","55"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","600","600","600","600","500"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","","Hermeetiline pöördkompressor","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10","-10","-10","-10","-10","","-10","","-10"]
["","","","Max","°CDB","50","50","50","50","50 (1)","","50","","46"]
["","Küte","Keskkond","Min","°CWB","-21","-21","-21","-21","-21 (1)","","-21","","-15"]
["","","","Max","°CWB","18","18","18","18","18","","18","","18"]
["Mürarõhutase","Jahutus","","Nom","dBA","46","46","47","48","48","","48","","47"]
["","Küte","","Nom","dBA","47","47","49","49","49","","49","","48"]
["Külmaaine","Tüüp","","","","R-32","R-32","R-32","R-32","R-32","","R-32","","R-32"]
["","Kogus","","","kg","0.95","0.95","0.95","0.95","1.10","","1.15","","1.15"]
["","Kogus","","","tCO2Eq","0.65","0.65","0.65","0.65","0.75","","0.78","","0.78"]
["","GWP","","","","675","675","675","675","675","","675","","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20","20","20","30","30","","30","","30"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","","0,02 (torustikule, mille pikkus ületab 10 m)","","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15","15","15","20","20","","20","","20"]
["Energiatõhususe klass","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Elektritoide","Faas","","","","1~","1~","1~","1~","1~","","1~","","1~"]
["","Sagedus","","","Hz","50","50","50","50","50","","50","","50"]
["","Pinge","","","V","220-240","220-240","220-240","220-240","220-240","","220-240","","220-240"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","1","1","1","1"]
["","Tühjendusliitmik","","","","1","1","1","1","1"]
["","Külmutusagensi täitmise silt","","","","1","1","1","1","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","1","1","1","1","1"]
["","Üldised ohutusmeetmed","","","","1","1","1","1","1"]
["","LOT10 energiamärgistus","","","","1","1","1","1","1"]
["","Tühjendusava kate","","","","3","3","3","3","1"]
["Märkused","","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist","","(1) - Vt töövahemiku kohta eraldi joonist","","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","","(2) - Vt eraldi elektriandmete joonist","","(2) - Vt eraldi elektriandmete joonist"]
["","","","","","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase","","(3) - Sisaldav fluoritud kasvuhoonegaase","","(3) - Sisaldav fluoritud kasvuhoonegaase"]
["Standardsed lisatarvikud","Installation manual","","","","","","","","","","1","","1"]
["","Refrigerant charge label","","","","","","","","","","1","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","","","","","","1","","1"]
["","Drain cap","","","","","","","","","","3","","3"]
["","Drain plug","","","","","","","","","","1","","1"]