{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP71N5V1B9 (Archived)"]
["Mõõtmed","Ühik","","Kõrgus","mm","556","556","556","734","734"]
["","","","Laius","mm","740","740","740","954","954"]
["","","","Sügavus","mm","343","343","343","401","401"]
["Kaal","Ühik","","","kg","24","24","26","46","50"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10","-10","-10"]
["","","","Max","°CDB","48","48","48"]
["","Küte","Keskkond","Min","°CWB","-15","-15","-15"]
["","","","Max","°CWB","18","18","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","46","46","48"]
["","","","Nom","dBA","","","","47","52"]
["","Küte","","kiire","dBA","47","47","48"]
["","","","Nom","dBA","","","","49","52"]
["Külmaaine","Tüüp","","","","R-32","R-32","R-32","R-32","R-32"]
["","Kogus","","","kg","0.55","0.55","0.70","0.9","1.15"]
["","Kogus","","","tCO2Eq","0.37","0.37","0.48","0.61","0.78"]
["","GWP","","","","675.0","675.0","675.0","675","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20","20","20","30","30"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","12","12","12","20","20"]
["Standardsed lisatarvikud","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Elektritoide","Faas","","","","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240","220-240","220-240"]
["Kompressor","Tüüp","","","","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Standardsed lisatarvikud","Drain cap","","","","","","","3"]
["Energiatõhususe klass","","","","","","","","A+++ ~ D","A+++ ~ D"]
["Märkused","","","","","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist"]
["","","","","","","","","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","","","","","1"]
["","Külmutusagensi täitmise silt","","","","","","","","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","","","","","1"]
["","Tühjendusava kate","","","","","","","","3"]
["","Tühjendusava kork","","","","","","","","1"]