{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Mürarõhutase","Küte","","kiire","dBA","49","","","52"]
["","","","aeglane","dBA","46","","","49"]
["","Jahutus","","aeglane","dBA","46","","","49"]
["","","","kiire","dBA","49","","","52"]
["Standardsed lisatarvikud","Tühjendusava","","","","1","","","1"]
["","Paigaldusjuhend","","","","1","","","1"]
["Külmaaine","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Charge","","","kg","1.5","","","2.3"]
["","Tüüp","","","","R-410A","","","R-410A"]
["Toruühendused","Kõrguste vahe","IU - OU","Max","m","20","","","20"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","","","0,02 (torustikule, mille pikkus ületab 10 m)"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","","","Hermeetiline pöördkompressor"]
["Mõõtmed","Ühik","","Laius","mm","825","","","900"]
["","","","Sügavus","mm","300","","","320"]
["","","","Kõrgus","mm","735","","","770"]
["Kaal","Ühik","","","kg","48","","","71"]
["Power supply","Phase","","","","1~","","","1~"]
["","Sagedus","","","Hz","50","","","50"]
["","Pinge","","","V","220-240","","","220-240"]
["Märkused","","","","","(1) - SL: Õhuvoo seade, mis tagab ventilaatori vaikse töö","(1) - 220V","","(1) - SL: Õhuvoo seade, mis tagab ventilaatori vaikse töö","(1) - 220V"]
["","","","","","(2) - Sisaldav fluoritud kasvuhoonegaase","(2) - 230 V","","(2) - Sisaldav fluoritud kasvuhoonegaase","(2) - 230 V"]
["Mõõtmed","Ühik","","Kõrgus","mm","","735","735","","770","770"]
["","","","Laius","mm","","825","825","","900","900"]
["","","","Sügavus","mm","","300","300","","320","320"]
["Kaal","Ühik","","","kg","","48","48","","71","71"]
["Kompressor","Tüüp","","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","","-10","-10","","-10","-10"]
["","","","Max","° CDB","","46","46","","46","46"]
["","Küte","Keskkond","Min","°CWB","","-15","-15","","-15","-15"]
["","","","Max","°CWB","","18","20","","18","20"]
["Mürarõhutase","Jahutus","","kiire","dBA","","49","49","","52","52"]
["","","","aeglane","dBA","","46","46","","49","49"]
["","Küte","","kiire","dBA","","49","49","","52","52"]
["","","","aeglane","dBA","","46","46","","49","49"]
["Külmaaine","Tüüp","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Kogus","","","kg","","1.5","1.5","","2.3","2.3"]
["","Kogus","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","","30","30","","30","30"]
["","Jahutusaine lisatäide","","","kg/m","","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","","20","20","","20","20"]
["Standardsed lisatarvikud","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Elektritoide","Faas","","","","","1~","1~","","1~","1~"]
["","Sagedus","","","Hz","","50","50","","50","50"]
["","Pinge","","","V","","220-240","220-240","","220-240","220-240"]
["Märkused","","","","","","(3) - 240V","","","(3) - 240V"]
["Standardsed lisatarvikud","Drain socket","","","","","","1","","","1"]
["Müratase","Jahutamine","","","dBA","","","","65"]