{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","46.0"]
["","","Soojendamine","Ülimadal","m³/min","46.0"]
["","","","Ülimadal","cfm","1624"]
["","","Soojendamine","Ülimadal","cfm","1624"]
["Mõõtmed","Ühik","","Kõrgus","mm","770"]
["","","","Laius","mm","900"]
["","","","Sügavus","mm","320"]
["Kaal","Ühik","","","kg","71"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","730"]
["","","Soojendamine","Ülimadal","p/min","730"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","-10"]
["","","","Max","° CDB","46"]
["","Küte","Keskkond","Min","°CWB","-15"]
["","","","Max","°CWB","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","52"]
["","Küte","","kiire","dBA","52"]
["Külmaaine","Tüüp","","","","R-410A"]
["","Kogus","","","kg","2.3"]
["","Kogus","","","tCO2Eq","4.8"]
["","GWP","","","","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","30"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","20"]
["Standardsed lisatarvikud","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Elektritoide","Faas","","","","1~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","220-240"]
["Märkused","","","","","(1) - 220V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240V"]