{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Helirõhu tase","Küte","","kiire","dBA","47","","47","","48","48","48"]
["","Jahutus","","kiire","dBA","46","","46","","48","48","48"]
["Standardsed lisatarvikud","Liides (äravool)","","","","1","","1"]
["","Paigaldusjuhend","","","","1","","1","","1","1","1"]
["Jahutusaine","Charge","","","tCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Täide","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Tüüp","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Ventilaatorimootor","Kiirus","Jahutus","Ülimadal","p/min","780","","780","","780","790","670"]
["","","Küte","Ülimadal","p/min","740","","740","","740","780","670"]
["Toruühendused","Kõrguste vahe","IU - OU","Max","m","15","","15","","15","15","20"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","","0,02 (torustikule, mille pikkus ületab 10 m)","","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","","Hermeetiline pöördkompressor","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Mõõtmed","Ühik","","Laius","mm","765","","765","","765","765","825"]
["","","","Sügavus","mm","285","","285","","285","285","300"]
["","","","Kõrgus","mm","550","","550","","550","550","735"]
["Kaal","Ühik","","","kg","34","","34","","34","39","47"]
["Ventilaator","Õhu voolukiirus","Küte","Ülimadal","cfm","","","","","904","960","1,522"]
["","","Jahutus","Ülimadal","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Phase","","","","1~","","1~","","1~","1~","1~"]
["","Sagedus","","","Hz","50","","50","","50","50","50"]
["","Pinge","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Märkused","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: Õhuvoo seade, mis tagab ventilaatori vaikse töö","","(4) - SL: Õhuvoo seade, mis tagab ventilaatori vaikse töö","","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase"]
["","","","","","(5) - Sisaldav fluoritud kasvuhoonegaase","","(5) - Sisaldav fluoritud kasvuhoonegaase"]
["Mõõtmed","Ühik","","Kõrgus","mm","","550","","550"]
["","","","Laius","mm","","765","","765"]
["","","","Sügavus","mm","","285","","285"]
["Kaal","Ühik","","","kg","","34","","34"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","","780","","780"]
["","","Soojendamine","Ülimadal","p/min","","740","","740"]
["Kompressor","Tüüp","","","","","Hermeetiline pöördkompressor","","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","","-10","","-10"]
["","","","Max","°CDB","","46","","46"]
["","Küte","Keskkond","Min","°CWB","","-15","","-15"]
["","","","Max","°CWB","","18","","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","","46","","46"]
["","Küte","","kiire","dBA","","47","","47"]
["Külmaaine","Tüüp","","","","","R-410A","","R-410A"]
["","Kogus","","","kg","","1.0","","1.0"]
["","Kogus","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","","20","","20"]
["","Jahutusaine lisatäide","","","kg/m","","0,02 (torustikule, mille pikkus ületab 10 m)","","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","","15","","15"]
["Standardsed lisatarvikud","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Elektritoide","Faas","","","","","1~","","1~"]
["","Sagedus","","","Hz","","50","","50"]
["","Pinge","","","V","","220-240","","220-240"]
["Standardsed lisatarvikud","Tühjendusava kork","","","","","","","","1","1","1"]