{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Helirõhu tase","Küte","","kiire","dBA","47","47","48","48"]
["","Jahutus","","kiire","dBA","46","46","48","48"]
["Standardsed lisatarvikud","Tühjendusava kate","","","","1","1","","1"]
["","Paigaldusjuhend","","","","1","1","1","1"]
["","Külmutusagensi täitmise silt","","","","1","1","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","1","1","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid"]
["Jahutusaine","Charge","","","tCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Täide","","","kg","1.0","1.0","1.20","1.3"]
["","Tüüp","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilaatorimootor","Kiirus","Jahutus","Ülimadal","p/min","780","780","780","790"]
["","","Küte","Ülimadal","p/min","740","740","740","780"]
["Töövahemik","Jahutus","Keskkond","Max","°CDB","46","46","46","46"]
["","","","Min","°CDB","-10","-10","-10","-10"]
["","Küte","Keskkond","Max","°CWB","18","18","18","18"]
["","","","Min","°CWB","-15","-15","-15","-15"]
["Toruühendused","Kõrguste vahe","IU - OU","Max","m","","","15"]
["","Jahutusaine lisatäide","","","kg/m","","","0,020 (torustikule, mille pikkus ületab 10 m)"]
["Mõõtmed","Ühik","","Laius","mm","765","765","765","765"]
["","","","Sügavus","mm","285","285","285","285"]
["","","","Kõrgus","mm","550","550","550","550"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Kaal","Ühik","","","kg","34","34","34","39"]
["Ventilaator","Õhu voolukiirus","Küte","Ülimadal","cfm","904","904","904","960"]
["","","","Ülimadal","m³/min","25.6","25.6","25.6","27.2"]
["","","Jahutus","Ülimadal","m³/min","30.1","30.1","30.1","30.6"]
["","","","Ülimadal","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240","220-240"]
["Märkused","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase"]
["Standardsed lisatarvikud","Tühjendusava kork","","","","","","1"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","","","","","48.9","45.0"]
["","","Soojendamine","Ülimadal","m³/min","","","","","43.1","46.3"]
["","","","Ülimadal","cfm","","","","","1727","1589"]
["","","Soojendamine","Ülimadal","cfm","","","","","1522","1635"]
["Mõõtmed","Ühik","","Kõrgus","mm","","","","","735","735"]
["","","","Laius","mm","","","","","825","825"]
["","","","Sügavus","mm","","","","","300","300"]
["Kaal","Ühik","","","kg","","","","","47","48"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","","","","","670"]
["","","Soojendamine","Ülimadal","p/min","","","","","670"]
["Kompressor","Tüüp","","","","","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","","","","","-10","-10"]
["","","","Max","°CDB","","","","","46","46"]
["","Küte","Keskkond","Min","°CWB","","","","","-15","-15"]
["","","","Max","°CWB","","","","","18","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","","","","","48","49"]
["","","","aeglane","dBA","","","","","44","46"]
["","Küte","","kiire","dBA","","","","","48","49"]
["","","","aeglane","dBA","","","","","45","46"]
["Külmaaine","Tüüp","","","","","","","","R-410A","R-410A"]
["","Kogus","","","kg","","","","","1.7","1.5"]
["","Kogus","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","","","","","30","30"]
["","Jahutusaine lisatäide","","","kg/m","","","","","0,020 (torustikule, mille pikkus ületab 10 m)","0,020 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","","","","","20.0","20"]
["Standardsed lisatarvikud","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Elektritoide","Faas","","","","","","","","1~","1~"]
["","Sagedus","","","Hz","","","","","50","50"]
["","Pinge","","","V","","","","","220-230-240","220-230-240"]
["Märkused","","","","","","","","","","(1) - 230 V"]