{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Mürarõhutase","Küte","","kiire","dBA","","","48"]
["","Jahutus","","kiire","dBA","","","48"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","","","1"]
["","Külmutusagensi täitmise silt","","","","","","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","","","1"]
["","Tühjenduskork (ainult soojuspumbaga mudelitel)","","","","","","1"]
["Jahutusaine","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Charge","","","kg","","","1.2"]
["","Tüüp","","","","","","R-410A"]
["Ventilaatori mootor","Kiirus","Jahutus","Ülimadal","p/min","","","780"]
["","","Küte","Ülimadal","p/min","","","740"]
["Töövahemik","Jahutus","Keskkond","Max","° CDB","","","46"]
["","","","Min","° CDB","","","-10"]
["","Küte","Keskkond","Max","°CWB","","","18"]
["","","","Min","°CWB","","","-15"]
["Toruühendused","Kõrguste vahe","IU - OU","Max","m","","","15"]
["","Jahutusaine lisatäide","","","kg/m","","","0,02 (torustikule, mille pikkus ületab 10 m)"]
["Mõõtmed","Ühik","","Laius","mm","","","765"]
["","","","Sügavus","mm","","","285"]
["","","","Kõrgus","mm","","","550"]
["Kompressor","Tüüp","","","","","","Hermeetiline pöördkompressor"]
["Kaal","Ühik","","","kg","","","34"]
["Ventilaator","Õhu vooluhulk","Küte","Ülimadal","cfm","","","904"]
["","","","Ülimadal","m³/min","","","25.6"]
["","","Jahutus","Ülimadal","m³/min","","","30.1"]
["","","","Ülimadal","cfm","","","1,063"]
["Power supply","Phase","","","","","","1~"]
["","Sagedus","","","Hz","","","50"]
["","Pinge","","","V","","","220-240"]
["Märkused","","","","","","","(1) - SL: Õhuvoo seade, mis tagab ventilaatori vaikse töö"]
["Ventilaator","Õhu vooluhulk","Jahutamine","Ülimadal","m³/min","30.1","30.1"]
["","","Soojendamine","Ülimadal","m³/min","25.6","25.6"]
["","","","Ülimadal","cfm","1063","1063"]
["","","Soojendamine","Ülimadal","cfm","904","904"]
["Mõõtmed","Ühik","","Kõrgus","mm","550","550"]
["","","","Laius","mm","765","765"]
["","","","Sügavus","mm","285","285"]
["Kaal","Ühik","","","kg","34","34"]
["Ventilaatori mootor","Kiirus","Jahutamine","Ülimadal","p/min","780","780"]
["","","Soojendamine","Ülimadal","p/min","740","740"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","-10","-10"]
["","","","Max","° CDB","46","46"]
["","Küte","Keskkond","Min","°CWB","-15","-15"]
["","","","Max","°CWB","18","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","46","46"]
["","Küte","","kiire","dBA","47","47"]
["Külmaaine","Tüüp","","","","R-410A","R-410A"]
["","Kogus","","","kg","1.0","1.0"]
["","Kogus","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","20","20"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["","Kõrguste vahe","IU - OU","Max","m","15","15"]
["Standardsed lisatarvikud","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Elektritoide","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]
["Märkused","","","","","(1) - 220V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240V"]
["Standardsed lisatarvikud","Drain plug (only heat pump models)","","","","","1"]