{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N8"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B8","RXTP35N2V1B8"]
["Mürarõhutase","Küte","","Nom","dBA","49","49"]
["","Jahutus","","Nom","dBA","48","48"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","1"]
["","Külmutusagensi täitmise silt","","","","1","1"]
["","Mitmekeelsed fluorineeritud kasvuhoonegaaside sildid","","","","1","1"]
["Jahutusaine","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Kogus","","","kg","1.1","1.1"]
["","Tüüp","","","","R-32","R-32"]
["Ventilaatori mootor","Kiirus","Jahutus","Ülimadal","p/min","450","450"]
["","","Küte","Ülimadal","p/min","360","360"]
["Toruühendused","Kõrguste vahe","IU - OU","Max","m","15","15"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 10 m)","0,02 (torustikule, mille pikkus ületab 10 m)"]
["Compressor","Type","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Mõõtmed","Ühik","","Laius","mm","763","763"]
["","","","Sügavus","mm","312","312"]
["","","","Kõrgus","mm","551","551"]
["Kaal","Ühik","","","kg","38","38"]
["Power supply","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]
["Märkused","","","","","(1) - Sisaldav fluoritud kasvuhoonegaase","(1) - Sisaldav fluoritud kasvuhoonegaase"]
["","","","","","(2) - Vt töövahemiku kohta eraldi joonist","(2) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","(3) - Vt eraldi elektriandmete joonist","(3) - Vt eraldi elektriandmete joonist"]