{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Mürarõhutase","Küte","","kiire","dBA","","","48","48","50","50"]
["","Jahutus","","kiire","dBA","","","48","48","49","49"]
["Standardsed lisatarvikud","Kasutusjuhend","","","","","","1","1","1","1"]
["","Paigaldusjuhend","","","","","","1","1","1","1"]
["Jahutusaine","GWP","","","","","","675","675","675","675"]
["","Täide","","","kg","","","1.34","1.34","1.34","1.34"]
["","Tüüp","","","","","","R-32","R-32","R-32","R-32"]
["Töövahemik","Jahutus","Keskkond","Max","°CDB","","","43","43","43","43"]
["","","","Min","°CDB","","","-10","-10","-10","-10"]
["","Küte","Keskkond","Max","°CWB","","","18","18","18","18"]
["","","","Min","°CWB","","","-20","-20","-20","-20"]
["Torustikuühendused","Kõrguste vahe","IU - OU","Max","m","","","8","8","8","8"]
["Mõõtmed","Ühik","","Laius","mm","","","795","795","795","795"]
["","","","Sügavus","mm","","","300","300","300","300"]
["","","","Kõrgus","mm","","","693","693","693","693"]
["Kompressor","Tüüp","","","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Kaal","Ühik","","","kg","","","50","50","50","50"]
["Power supply","Faas","","","","","","1~","1~","1~","1~"]
["","Sagedus","","","Hz","","","50","50","50","50"]
["","Pinge","","","V","","","220-240","220-240","220-240","220-240"]
["Märkused","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase","(4) - Sisaldav fluoritud kasvuhoonegaase"]
["Mõõtmed","Ühik","","Kõrgus","mm","693","693"]
["","","","Laius","mm","795","795"]
["","","","Sügavus","mm","300","300"]
["Kaal","Ühik","","","kg","50","50"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-10","-10"]
["","","","Max","°CDB","43","43"]
["","Küte","Keskkond","Min","°CWB","-20","-20"]
["","","","Max","°CWB","18","18"]
["Mürarõhutase","Jahutus","","kiire","dBA","46","46"]
["","Küte","","kiire","dBA","46","46"]
["Külmaaine","Tüüp","","","","R-32","R-32"]
["","Kogus","","","kg","1.34","1.34"]
["","Kogus","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","10","10"]
["","Kõrguste vahe","IU - OU","Max","m","8","8"]
["Standardsed lisatarvikud","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Elektritoide","Faas","","","","1~","1~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","220-240","220-240"]