{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Mõõtmed","Ühik","","Kõrgus","mm","870","870"]
["","","","Laius","mm","1,100","1,100"]
["","","","Sügavus","mm","460","460"]
["Kaal","Ühik","","","kg","117","117"]
["Kompressor","Tüüp","","","","Hermeetiline spiraalkompressor","Hermeetiline spiraalkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-20","-20"]
["","","","Max","°CDB","46","46"]
["","Küte","Keskkond","Min","°CWB","-20","-20"]
["","","","Max","°CWB","15","15"]
["Müratase","Jahutamine","","","dBA","73","76"]
["","Soojendamine","","","dBA","76 (1)","79 (1)"]
["Helirõhu tase","Jahutus","","Nom","dBA","53","57"]
["","Küte","","Nom","dBA","60","63"]
["Jahutusaine","Tüüp","","","","R-32","R-32"]
["","Täide","","","kg","5","5"]
["","GWP","","","","675","675"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52","9.52"]
["","Gaas","","Välisdiameeter","mm","22.2","22.2"]
["","Torustiku pikkus","Max","OU - IU","m","100","100"]
["","","Süsteem","Täiteta","m","30","30"]
["","Jahutusaine lisatäide","","","kg/m","Vaadake paigaldusjuhendit","Vaadake paigaldusjuhendit"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1","1"]
["","Üldised ohutusmeetmed","","","","1","1"]
["","Kaablisidemed","","","","2","2"]
["","Mahakooritav F-gaasi märgis","","","","1","1"]
["","Ühendustorud","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Sagedus","","","Hz","50","50"]
["","Pinge","","","V","380-415","380-415"]
["Vool - 50Hz","Kaitsme maksimaalne nimivool (MFA)","","","A","20","20"]
["Märkused","","","","","(1) - Vastavalt määrusele ENER Lot 21","(1) - Vastavalt määrusele ENER Lot 21"]