{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Mõõtmed","Ühik","","Kõrgus","mm","734","734","734"]
["","","","Laius","mm","870","870","870"]
["","","","Sügavus","mm","373","373","373"]
["Kaal","Ühik","","","kg","52","52","52"]
["Kompressor","Tüüp","","","","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor","Hermeetiline pöördkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","°CDB","-20","-20","-20"]
["","","","Max","°CDB","52","52","52"]
["","Küte","Keskkond","Min","°CWB","-21","-21","-21"]
["","","","Max","°CWB","18","18","18"]
["Helivõimsustase","Jahutamine","","","dBA","62","63","64"]
["","Soojendamine","","","dBA","62","63","64"]
["Mürarõhutase","Jahutus","","Nom","dBA","48","49","50"]
["","Küte","","Nom","dBA","48","49","50"]
["Külmaaine","Tüüp","","","","R-32","R-32","R-32"]
["","Kogus","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Kogus","","","tCO2Eq","1.05","1.05","1.05"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","6.35","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","9.52","12.7","12.7"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","50","50","50"]
["","Jahutusaine lisatäide","","","kg/m","0,02 (torustikule, mille pikkus ületab 30 m)","0,02 (torustikule, mille pikkus ületab 30 m)","0,02 (torustikule, mille pikkus ületab 30 m)"]
["","Kõrguste vahe","IU - OU","Max","m","30","30","30"]
["Standardsed lisatarvikud","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Elektritoide","Faas","","","","1~","1~","1~"]
["","Sagedus","","","Hz","50","50","50"]
["","Pinge","","","V","220-240","220-240","220-240"]
["Märkused","","","","","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist","(1) - Vt töövahemiku kohta eraldi joonist"]
["","","","","","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist","(2) - Vt eraldi elektriandmete joonist"]
["","","","","","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase","(3) - Sisaldav fluoritud kasvuhoonegaase"]
["Standardsed lisatarvikud","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]