{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Mõõtmed","Ühik","","Kõrgus","mm","1,680"]
["","","","Laius","mm","930"]
["","","","Sügavus","mm","765"]
["Kaal","Ühik","","","kg","183.0"]
["Kompressor","Tüüp","","","","Hermeetiline spiraalkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","-5.0"]
["","","","Max","° CDB","46.0"]
["","Küte","Keskkond","Min","°CWB","-15.0"]
["","","","Max","°CWB","15.0"]
["Müratase","Jahutamine","","","dBA","78.0"]
["","Soojendamine","","","dBA","78.0"]
["Külmaaine","Tüüp","","","","R-410A"]
["","Charge","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","9.52"]
["","Gaas","","Välisdiameeter","mm","22.2"]
["","Torustiku pikkus","Max","OU - IU","m","100"]
["","","Süsteem","Täiteta","m","30"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1"]
["","Ühendustorud","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","380-415"]
["Vool - 50Hz","Kaitsme maksimaalne nimivool (MFA)","","","A","25"]
["Märkused","","","","","(1) - FDQ siseseadme elektritoide on eraldi"]
["","","","","","(2) - Vt eraldi elektriandmete jooniseid"]
["Mõõtmed","Ühik","","Kõrgus","mm","","1680"]
["","","","Laius","mm","","930"]
["","","","Sügavus","mm","","765"]
["Kaal","Ühik","","","kg","","184.0"]
["Kompressor","Tüüp","","","","","Hermeetiliselt suletud spiraalkompressor"]
["Töövahemik","Jahutus","Keskkond","Min","° CDB","","-5.0"]
["","","","Max","° CDB","","46.0"]
["","Küte","Keskkond","Min","°CWB","","-15.0"]
["","","","Max","°CWB","","15.0"]
["Helivõimsustase","Jahutamine","","","dBA","","78.0"]
["","Soojendamine","","","dBA","","78.0"]
["Külmaaine","Kogus","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Kogus","","","tCO2Eq","","19.4"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","12.70"]
["","Gaas","","Välisdiameeter","mm","","22.2"]
["Torustikuühendused","Torustiku pikkus","Max","OU - IU","m","","100"]
["","","Süsteem","Täiteta","m","","30"]
["Standardsed lisatarvikud","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Elektritoide","Sagedus","","","Hz","","50"]
["Vool – 50 Hz","Kaitsme maksimaalne nimivool (MFA)","","","A","","25"]