{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Mürarõhutase","Küte","","kiire","dBA","39"]
["","","","Keskmine","dBA","34"]
["","","","Vaikne töö","dBA","20"]
["","","","aeglane","dBA","26"]
["","Jahutus","","Keskmine","dBA","33"]
["","","","Vaikne töö","dBA","19"]
["","","","aeglane","dBA","25"]
["","","","kiire","dBA","41"]
["Standardsed lisatarvikud","Paigaldusjuhend","","","","1"]
["","Kasutusjuhend","","","","1"]
["","Traadita juhtimispult","","","","1"]
["","AAA kuivelement patareid","","","","2"]
["","Kaugjuhtimispuldi hoidik","","","","1"]
["","Paigaldusplaat","","","","1"]
["","Titaanapatiidist deodoriseeriv filter","","","","1"]
["","Siseseadme kinnituskruvid","","","","2"]
["","WLAN-adapteri komplekt","","","","1"]
["Juhtimissüsteemid","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Torustikuühendused","Vedelik","","Välisdiameeter","mm","6.35"]
["","Gaas","","Välisdiameeter","mm","9.50"]
["","Tühjendus","","","","18"]
["Sisendvõimsus","Jahutus","","Nom","kW","0.029"]
["","Küte","","Nom","kW","0.023"]
["Sound power level","Jahutamine","","","dBA","58"]
["","Soojendamine","","","dBA","55"]
["Mõõtmed","Ühik","","Laius","mm","778"]
["","","","Sügavus","mm","272"]
["","","","Kõrgus","mm","295"]
["Korpus","Värvus","","","","Valge"]
["Kaal","Ühik","","","kg","10.0"]
["Ventilaator","Õhu vooluhulk","Küte","kiire","m³/min","9.3"]
["","","","Keskmine","m³/min","8.2"]
["","","","aeglane","m³/min","6.2"]
["","","","Vaikne töö","m³/min","5.1"]
["","","Jahutus","aeglane","m³/min","5.7"]
["","","","Keskmine","m³/min","7.5"]
["","","","kiire","m³/min","10.5"]
["","","","Vaikne töö","m³/min","4.3"]
["Power supply","Faas","","","","1~"]
["","Nimetus","","","","V1"]
["","Sagedus","","","Hz","50"]
["","Pinge","","","V","220-240"]
["Märkused","","","","","(1) - Jahutus: sisetemp. 27 °CDB, 19,0 °CWB; välistemp. 35 °CDB, 24 °CWB; ekvivalentne torustiku pikkus: 5 m"]
["","","","","","(2) - Küte: sisetemp. 20 °CDB; välistemp. 7 °CDB, 6 °CWB; ekvivalentne jahutustorustik: 5 m"]
["Sisendvõimsus","Jahutus","","Nom","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Küte","","Nom","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Korpus","Värvus","","","","","Valge","Valge","Valge","Valge","Valge","Valge","Valge"]
["Mõõtmed","Ühik","","Kõrgus","mm","","295","295","295","295","295","295","299"]
["","","","Laius","mm","","778","778","778","778","778","778","998"]
["","","","Sügavus","mm","","272","272","272","272","272","272","292"]
["Kaal","Ühik","","","kg","","10","10","10","10","10","10","14.5"]
["Ventilaator","Õhu vooluhulk","Jahutus","kiire","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","Õhuvoolu kiirus","Jahutus","Keskmine","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","aeglane","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Vaikne töö","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Küte","kiire","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","Õhuvoolu kiirus","Küte","Keskmine","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","Küte","aeglane","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Vaikne töö","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Helivõimsustase","Jahutamine","","","dBA","","58","58","58","58","58","58","58"]
["","Soojendamine","","","dBA","","55","55","55","55","55","55","58"]
["Mürarõhutase","Jahutus","","kiire","dBA","","41","41","41","41","45","45","44"]
["Helirõhu tase","Jahutus","","Keskmine","dBA","","33","33","33","33","33","33","40"]
["Mürarõhutase","Jahutus","","aeglane","dBA","","25","25","25","25","25","25","36"]
["","","","Vaikne töö","dBA","","19","19","19","19","19","19","27"]
["","Küte","","kiire","dBA","","39","39","39","39","39","39","43"]
["Helirõhu tase","Küte","","Keskmine","dBA","","34","34","34","34","35","35","39"]
["Mürarõhutase","Küte","","aeglane","dBA","","26","26","27","27","28","28","34"]
["","","","Vaikne töö","dBA","","20","20","20","20","20","20","31"]
["Toruühendused","Vedelik","","Välisdiameeter","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gaas","","Välisdiameeter","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Tühjendus","","","","","18","18","18","18","18","18","18"]
["Juhtimissüsteemid","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["Juhtsüsteemid","Juhtmega kaugjuhtimine","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardsed lisatarvikud","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Elektritoide","Nimetus","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Faas","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Sagedus","","","Hz","","50","50","50","50","50","50","50"]
["","Pinge","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardsed lisatarvikud","Silver particle filter","","","","","","","","","","","1"]